**Paper clip factory – Paper clip**

**Properties:**

Type: Cradle-Gate Nation: World Version: V0

**Chapter 1: Life Cycle Inventory**

|  |  |  |  |
| --- | --- | --- | --- |
|  | Tutorial Model <LC> | | |
| SUM | Tutorial End of Life Model <LC> | DE: BF Steel billet / slab / bloom ts <p-agg> |
| DE: EAF Steel billet / Slab / Bloom ts <p-agg> |  |
| Inputs | 124.1 | 53.9 | 70.2 |
| Resources | 124.1 | 53.9 | 70.2 |
| Energy resources | 114.5 | 50.7 | 63.8 |
| Non renewable energy resources | 114.5 | 50.7 | 63.8 |
| Crude oil (resource) | 27.7 | 9.6 | 18.1 |
| Crude oil (in MJ) | 8.7 | 5.8 | 2.9 |
| Oil sand (10% bitumen) (in MJ) | 10.4 | 2.5 | 7.9 |
| Oil sand (100% bitumen) (in MJ) | 8.6 | 1.3 | 7.3 |
| Hard coal (resource) | 24.3 | 12.8 | 11.5 |
| Lignite (resource) | 12.2 | 3.8 | 8.4 |
| Natural gas (resource) | 24.1 | 10.4 | 13.7 |
| Peat (resource) | 14.1 | 7.2 | 6.9 |
| Uranium (resource) | 12.1 | 6.9 | 5.2 |
| Material resources | 9.6 | 3.2 | 6.4 |
| Non renewable elements | 9.6 | 3.2 | 6.4 |
| Antimony | 9.6 | 3.2 | 6.4 |

图形用户界面

低可信度描述已自动生成